Cutting Instructions

* if cutting smaller width rolls it is important to completely fill shaft
* if cutting smaller roll(s) than shaft width, it is important to place rolls toward ends of shaft and NOT in middle. (see picture)
* if cutting different size diameters, DO NOT place larger diameters in center or middle of smaller diameter rolls.  Larger diameter rolls should be placed at ends of shaft
* Silicone spray should be used to keep blade sharp and make cutting rolls easier
* Do not cut roll all at once
  + Cut approx 3” of paper and let paper fall and repeat till you reach the core

Depending on type of paper and width of rolls, blade may not always cut 100% to core but should be very close

